 **CLS Focus Micro T DMX – Track zoom spot**

|  |  |  |
| --- | --- | --- |
| Type | : | 1 Watt, 6°-90° track zoom spot |
| Colour | : | Black |
| Material | : | Coated Aluminium |
| Weight | : | 35 gr |
| IP Rating | : | IP20 |
| IK class | : | x |
| Optics | : | 6°-90° zoom optics |
| Light source | : | Lumileds High Power LED: 1x Luxeon Z ES |
| Colour Temperature | : | 2700K, 3000K, 3500K or 4000K |
| CRI | : | ≈95 |
| Drive current | : | 24VDC |
| Driver | : | Power supply external, DMX driver internal |
| Dimming | : | DMX 512 or Magno Dimming |
| Optional accessories | : | Stucchi MULTISYSTEM EVO |
| Connection | : | Stucchi MULTISYSTEM EVO track adapter |
| Remarks | : | Internal slot for correction/colour filters, 2 cuttable snoots included |
| Life time | : | Up to 50.000H, L90B10 |
| Warranty | : | 5 years warranty |
| Origin | : | Designed and Manufactured in The Netherlands |

**­­­**

****

