
**CLS Focus Track 230V Magno individually dimmable Spot**

|  |  |  |
| --- | --- | --- |
| Type | : | 6 Watt IP20 aluminium track 13°-65° zoom spot with Magno dimming |
| Colour | : | Black anodized aluminium and white coated |
| Material | : | CNC machined aluminium |
| Weight | : | 275 gr |
| IP Rating | : | IP20 |
| IK class | : | X |
| Optics | : | 13°-65° zoom lens |
| Light source | : | Lumileds High Power LED: 4x Luxeon Z ES |
| Colour temperature | : | 2700K, 3000K & 4000K |
| CRI | : | ≈95 |
| Power | : | 100 – 240 VAC |
| Driver | : | Internal power supply |
| Dimming | : | Magno dim system |
| Remarks | : | Magno dimming offers the facility of individually dimmable fixtures without the need for any control equipment  No extra cabling needed Calibration functionality  Internal slot for colour and/or correction filters |
| Optional accessories | : | Rail products, snoot, extension pipe of 10 & 30 cm |
| Connection | : | Multi Track adapter |
| Life time | : | Up to 50.000 hours |
| Warranty | : | 3 years |
| Origin | : | Designed and manufactured in the Netherlands |
|  |  |  |

****

****