**CLS Focus Track 230V Magno individually dimmable Spot**

|  |  |  |
| --- | --- | --- |
| Type |  : | 6 Watt IP20 aluminium track 13°-65° zoom spot with Magno dimming |
| Colour |  : | Black anodized aluminium and white coated |
| Material |  : | CNC machined aluminium |
| Weight |  : | 275 gr |
| IP Rating |  : | IP20 |
| IK class |  : | X |
| Optics |  : | 13°-65° zoom lens |
| Light source |  : | Lumileds High Power LED: 4x Luxeon Z ES |
| Colour temperature |  : | 2700K, 3000K & 4000K |
| CRI |  : | ≈95 |
| Power |  : | 100 – 240 VAC |
| Driver |  : | Internal power supply  |
| Dimming |  : | Magno dim system |
| Remarks |  : | Magno dimming offers the facility of individually dimmable fixtures without the need for any control equipmentNo extra cabling neededCalibration functionalityInternal slot for colour and/or correction filters |
| Optional accessories |  : | Rail products, snoot, extension pipe of 10 & 30 cm |
| Connection |  : | Multi Track adapter |
| Life time |  : | Up to 50.000 hours |
| Warranty |  : | 3 years |
| Origin |  : | Designed and manufactured in the Netherlands |
|  |  |  |

****

****