

**CLS Jade C semi-surface mounted spot**

|  |  |  |
| --- | --- | --- |
| Type | : | 20 Watt (2000 lm) or 30 Watt (3500 lm) semi-surface mounted spot |
| Colour | : | Configurable: Black, white or grey |
| Material | : | Coated aluminium & PC/ABS V0 |
| Weight | : | 780 gr |
| IP Rating | : | IP20 |
| IK class | : | x |
| Optics | : | Configurable: 19°, 37° or 63° beam angle |
| Light source | : | Citizen CoB LED module |
| Colour Temperature | : | 2700K, 3000K & 4000K |
| CRI | : | >80 or >90 |
| Driver | : | Internal power supply, 230V |
| Power factor | : | >0,90 |
| Dimming | : | Phase cut (mains dimmable), DALI dim or Local Dim through a potentiometer on housing |
| Remarks | : | Integrated soft diffusion filter |
| Optional accessories | : | X |
| Connection | : | 150 cm cable with schuko connector |
| Life time | : | Up to 50.000 hours |
| Warranty | : | 5 years warranty |
| Origin | : | Designed and manufactured in The Netherlands |
|  |  |  |
|  |  |  |

****

****