**CLS Jade C semi-surface mounted spot**

|  |  |  |
| --- | --- | --- |
| Type |  : | 20 Watt (2000 lm) or 30 Watt (3500 lm) semi-surface mounted spot |
| Colour |  : | Configurable: Black, white or grey  |
| Material |  : | Coated aluminium & PC/ABS V0 |
| Weight |  : | 780 gr |
| IP Rating |  : | IP20 |
| IK class |  : | x |
| Optics |  : | Configurable: 19°, 37° or 63° beam angle |
| Light source |  : | Citizen CoB LED module |
| Colour Temperature |  : | 2700K, 3000K & 4000K |
| CRI |  : | >80 or >90 |
| Driver |  : | Internal power supply, 230V |
| Power factor |  : | >0,90 |
| Dimming |  : | Phase cut (mains dimmable), DALI dim or Local Dim through apotentiometer on housing |
| Remarks |  : | Integrated soft diffusion filter |
| Optional accessories |  : | X |
| Connection |  : | 150 cm cable with schuko connector |
| Life time |  : | Up to 50.000 hours |
| Warranty |  : | 5 years warranty |
| Origin |  : | Designed and manufactured in The Netherlands |
|  |  |  |
|  |  |  |

****

****