 **CLS Focus Micro Spot**

|  |  |  |
| --- | --- | --- |
| Type |  : | 1 Watt, 6°-90° zoom spot |
| Colour |  : | Black |
| Material |  : | Coated Aluminium |
| Weight |  : | 20 gr |
| IP Rating |  : | IP20 |
| IK class |  : | x |
| Optics |  : | 6°-90° zoom optics |
| Light source |  : | Lumileds High Power LED: 1x Luxeon Z ES |
| Colour Temperature |  : | 2700K, 3000K, 3500K or 4000K |
| CRI |  : | ≈95 |
| Drive current |  : | Spot: 350mA |
| Driver |  : | Power supply external |
| Dimming |  : | 1-10V, DMX512, Bluetooth by Casambi |
| Optional accessories |  : | Magnetic foot mount |
| Connection |  : | SmartConnect System |
| Remarks |  : | Internal slot for correction/colour filters, 2 cuttable snoots included |
| Life time |  : | Up to 50.000H, L90B10 |
| Warranty |  : | 5 years warranty |
| Origin |  : | Designed and Manufactured in The Netherlands |

